1、访问限制
[image: image1.png]<Directory "/usr/local/awstats/wmmroot">

Options None
Allowoverride None

# Order allow,deny
# Allow from all
<RequireAll>
Require ip 192.168.199.1
# AuthName "111"
# AuthType Bas ic
# AuthUserFile /usr/local/httpd/conf/. awspud
# Require valid-user
# Require all granted
# Require not ip 192.168.199.1
</RequireAll>
B/Directory>

"/usr/local /httpd/conf/httpd.conf" Sd6L, 19440C

540,1

R
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Forbidden

You don't have permission fo access this resource.




[image: image3.png]-
<Directory "/usr/local/austats/wmroot">
Options None
Allowdverride None

# Order allow,deny
# Allow from all
<RequireAll>

Require ip 192.168.199.1
AuthName "111"
AuthType Basic
AuthUserFile /usr/local/httpd/conf/. awspud
Require valid-user
# Require all granted
# Require not ip 192.168.199.1
</Requireall>
</Directliry>
"/usr/local/httpd/conf/httpd.conf" 5d6L, 19436

540,9

R
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2、基于域名
[image: image5.png]<Directory />
Allowdverride none
#Require all denied
Require all granted
</Directory>




[image: image6.png]<VirtualHost *:80>
DocumentRoot “/html/aaa"
ServerName ww.aaa.com
ErrorLog "logs/asa.com-error_log"
CustonLog "logs/aaa. com-access_Log"
</VirtualHost>

<VirtualHost *:80>
DocumentRoot */html /bbb
ServerName_ww.bbb. com
ErrorLog "logs /bbb com-error_log"
BustonLog "logs/bbb. com-access_Log"
</VirtualHost>

common

common
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3、基于ip
[image: image9.png][root@localhost ~]# ifconfig

ens33: flags=4163<UP,BROADCAST,RUNNING, MULTICAST> mtu 1500

inet 192.168.199.10 netmask 255.255.255.0 broadcast 192.168.199.255
inet6 fe8o::de30:74d7:6fae:achs prefixlen 64 scopeid 0x20<link>
ether 00:0c:29:67:0d:ce txqueuelen 1000 (Ethernet)

RX packets 52897 bytes 16317024 (15.5 MiB)

RX errors 0 dropped 0 overruns 0 frame 0

TX packets 18813 bytes 2435808 (2.3 MiB)

TX errors © dropped © overruns © carrier © collisions 0

: flags=4163<UP ,BROADCAST ,RUNNING, MULTICAST> mtu 1500
inet 192.168.199.11 netmask 255.255.255.0 broadcast 192.168.199.255
ether 00:0c:29:67:0d:ce txqueuelen 1000 (Ethernet)

ens33:

: flags=4163<UP ,BROADCAST ,RUNNING, MULTICAST> mtu 1500
inet 192.168.199.12 netmask 255.255.255.0 broadcast 192.168.199.255
ether 00:0c:20:67:0d:ce txqueuelen 1000 (Ethernet)

ens33:
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4、基于端口
[image: image12.png]L
<VirtualHost 192.168.199.10:8008>

DocumentRoot “/html/aaa"

ServerName ww.aaa.com

ErrorLog "logs/asa.com-error_log"

CustonLog "logs/aza. con-access_Log" common
</VirtualHost>

<VirtualHost 192.168.199.10:80098
DocumentRoot */html /bbb
ServerName_ww.bbb. com
ErrorLog "logs /bbb com-error_log"
CustonLog "Logs/bbb. con-access_Log" common
</VirtualHost>
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