限制 1、要求仅客户机一台主机可以访问awstats网页！

[image: image1.png]#

# Directives to allow use of AWStats as a CGI

#

Alias /awstatsclasses "/usr/local/awstats/wwwroot/classes/"
Alias /awstatscss "/usr/local/awstats/wwwroot/css/"

Alias /awstatsicons "/usr/local/awstats/wwwroot/icon/"
Scripthlias /awstats/ */usr/local/awstats/wmroot/cgi-bin/"

<Directory */usr/local/austats /mmroot®>
Options None
Allowoverride None
# Require all granted
<RequireAll>
Require all granted
Require not ip 192.168.128.132
</RequireAll>
</Directory>

<Directory */usr/local/awstats /wawroot/cgi-bin">
Options +ExecCGI
Allow0verride None
#Require all granted
<RequireAll>
Require all granted
Require not ip 192.168.128.132
</RequireAll>

</Directory>

#<VirtualHost 192.168.128.100:80>
#  DocumentRoot */html/aaa"

# ServerName www.aaa.com

#  Errorlog "logs/aaa.con-error_log"

# Customlog "logs/aaa.com-access_log" common
#</VirtualHost>

#<VirtualHost 192.168.128.101:80>
#  DocumentRoot */html/bbb"

#  ServerName w.bbb.com
#  Errorlog "logs/bbb.com-error_log"

# Customlog "logs/bbb.com-access_log" common
#</VirtualHost>

#

# This is to permit URL access to scripts/files in AWStats directory.





 2、要求使用用户访问，用户名为自己的名字

[image: image2.png]:\Users\quF0X23>curl ~v -u qinquanjun:123 http://192. 168. 128. 30/awstats/awstats. pl fconfig=wm. qinquanjun. com
Trying 192.168. 128.30...

TCP_NODELAY set

Comnected to 192. 168, 128.30 (192. 168, 128.30) port 80 (#0)

Server auth using Basic with user ~qinquanjun’

GET /awstats/avstats. pl?contig=wm. qinquanjun. con HTTP/1. 1

Host: 192. 168. 128. 30

Authorization: Basic c¥lucKVhbmplbjaxliili=

User-Agent: curl/7.55.1

Accepts /%

HTTP/1.1 200 OK

Date: Thu, 10 Sep 2026 16:57:13 GHT

Server: Apache/2.4.46 (Unix)

Cache-Control: public

Expires: Thu Sep 10 16:57:13 2026
Last-Nodified: Thu, 10 Sep 2026 16:57:13 GNT
Content-Length: 1053

Content-Type: text/html; charset=uti-8
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虚拟主机 1、完成基于域名、IP、端口的虚拟主机，两个域名分别都是同名域名，必须安装DNS服务完成
[image: image3.png]> For more info, ctrl+click on help or visit our website

Last login: Fri Sep 11 00:41:45 2026 from 192.168.128.1
[root@localhost ~1# cat /usr/local/httpd/conf/extra/httpd-vhosts. conf
Virtual Hosts

Required modules: mod_log_config

If you want to maintain multiple domains/hostnames on your
machine you can setup VirtualHost containers for them. Most configurations
use only name-based virtual hosts so the server doesn't need to worry about
1P addresses. This is indicated by the asterisks in the directives below.

Please see the documentation at
<URL:http://httpd. apache.org/docs/2.4/vhosts />
for further details before you try to setup virtual hosts.

You may use the command line option '-S' to verify your virtual host
configuration.

VirtualHost example:
Almost any Apache directive may go into a VirtualHost container.
The first VirtualHost section 1s used for all requests that do not
match a ServerName or ServerAlias in any <VirtualHost> block.

T

#<Virtualhost *:80>
<VirtualHost 192.168.128.100:8888>

# Serveradnin webmaster@dummy-host. example.com

DocumentRoot "/html/aaa"

ServerName ww.aaa.com

# Serveralias www.dunmy-host. exanple.com

ErrorLog "logs/asa.com-error_Log"

CustonLog "logs/aaa. com-access_Log" common
</VirtualHost>

#<Virtualhost *:80>
<VirtualHost 192.168.128.100:6666>

# Serveradnin webmaster@dunmy-host2. example.com

DocumentRoot */html/bbb*

ServerName_www.bbb. com

ErrorLog "logs/bbb.com-error_log"

CustonLog "Logs/bbb.com-access_Log* common
</VirtualHost>
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IP :

[image: image6.png][root@localhost ~1# ifconfig ens33:1 192.168.128.100

[root@localhost ~I# ifconfig ens33:2 192.168,128.101

[root@localhost ~1# vim /usr/local /httpd/conf/extra/httpd-vhosts. conf

452 /var/spool /mail/root s

[root@localhost ~1# cat /usr/local/httpd/conf/extra/httpd-vhosts. conf
Virtual Hosts

Required modules: mod_log_config

If you want to maintain multiple domains/hostnames on your
machine you can setup VirtualHost containers for them. Most configurations
use only name-based virtual hosts so the server doesn't need to worry about
1P addresses. This is indicated by the asterisks in the directives below.

Please see the documentation at
<URL:http://httpd. apache.org/docs /2. 4/vhosts />
for further details before you try to setup virtual hosts.

You may use the command line option
configuration.

* to verify your virtual host

VirtualHost example:
Almost any Apache directive may go into a VirtualHost container.
The first VirtualHost section 1s used for all requests that do not
match a ServerName or ServerAlias in any <VirtualHost> block.

N N W W W W W W

#<Virtualhost *:80>
<VirtualHost 192.168.128.100:80>

# Serveradnin webmaster@dummy-host. example.com

DocumentRoot "/html/aaa"

ServerName ww.aaa.com

# Serveralias www.dunmy-host. exanple.com

ErrorLog "logs/asa.com-error_Log"

CustonLog "logs/aaa. com-access_Log" common
</VirtualHost>

#<Virtualhost *:80>
<VirtualHost 192.168.128.101:80>

# Serveradnin webmaster@dummy-host2. example.com

DocumentRoot */html/bbb*

ServerName_www.bbb. com

ErrorLog "logs/bbb.com-error_log"

CustonLog "Logs/bbb.com-access_Log* common
</VirtualHost>

[root@localhost ~]# systemctl stop httpd
[root@localhost ~]# systemctl restart httpd
[root@localhost ~1# I
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端口:

[image: image9.png]39 # other reason.

40 #

41 # Mutex default:logs

42

a3 #

44 # Listen: Allows you fo bind Apache to specific Ip addracacs and/or
45 # ports, instead of the default. See also the <JPiE

46 # directive.

a7 #

48 # Change this to Listen on specific IP addresses as shown below to
49 # prevent Apache from glomming onto all bound IP addresses.

50 #

51 #Listen 12.34.56.78:80

52 Listen 80

53 Listen 8888

54
55
56
57
58
59
60
61
62
63
64
65
66
67

Listen 6666

#

# Dynamic Shared Object (DSO) Support

#

# To be able to use the functionality of a module which was built as a DSO you
# have to place corresponding "LoadModule’ lines at this location so the

# directives contained in it are actually available _before_ they are used.
# Statically compiled modules (those listed by "httpd -1') do not need

# to be Loaded here.

#

# Example:

# LoadModule foo_module modules/mod_foo.so

#

LoadHodule authn_file_module modules/mod_authn_file.so

-0adlloduie authn_T1tle_mocdu'e modures/moc.

Jthn_f1ie.st





[image: image10.png][root@localhost ~]# cat /usr/local/httpd/conf/extra/httpd-vhosts.conf
Virtual Hosts

Required modules: mod_log_config

If you want to maintain multiple domains/hostnames on your
machine you can setup VirtualHost containers for them. Most configurations
use only name-based virtual hosts so the server doesn't need to worry about
1P addresses. This is indicated by the asterisks in the directives below.

Please see the documentation at
<URL:http://httpd. apache.org/docs/2.4/vhosts />
for further details before you try to setup virtual hosts.

You may use the command line option '-S' to verify your virtual host
configuration.

VirtualHost example:
Almost any Apache directive may go into a VirtualHost container.
The first VirtualHost section 1s used for all requests that do not
match a ServerName or ServerAlias in any <VirtualHost> block.

T

#<Virtualhost *:80>
<VirtualHost 192.168.128.100:8888>

# Serveradnin webmaster@dummy-host. example.com

DocumentRoot "/html/aaa"

ServerName ww.aaa.com

# Serveralias www.dunmy-host. exanple.com

ErrorLog "logs/asa.com-error_Log"

CustonLog "logs/aaa. com-access_Log" common
</VirtualHost>

#<Virtualhost *:80>
<VirtualHost 192.168.128.101:6666>

# Serveradnin webmaster@dummy-host2. example.com

DocumentRoot */html/bbb*

ServerName_www.bbb. com

ErrorLog "logs/bbb.com-error_log"

CustonLog "Logs/bbb.com-access_Log* common
</VirtualHost>
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