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Tdrn] MHIO at 0xfe000000 size is 256 kib

Idrn] global init.

ITIM] Zone kernel: Auailable graphics memory: 2013188 kiB
ITIM] Initializing pool allocator

ITIM] Initializing DA pool allocator

scsi_targeto Beginning Domain Validation

Idrn] Supports ublank timestanp caching Rev 2 (21.10.2013).

Idrn] No driver support for ublank timestamp query.

Idrn] Screen Target Display device initialized

Idrn] width 1280

Idrn] height 768

Idrn1 bpp 32

scsi target0:0:0: Domain Validation skipping urite tests

scsi targeto Ending Donain Validation

scsi targeto FAST-40 UIDE SCSI 8.0 MB/s ST (25 ns, offset 1

Idrn] Fifo max 0x00040000 min 0x00001000 cap 0x0000077f
Idrn] Using comnand buffers with DMA pool.

Idrn] DX: mo.

Idrn] Atonic: yes

fbcon: sugadenfb (£b0) is primary device

Console: suitching to colour frame buffer device 160x48

Idrn] Initialized unugfx 2.14.1 20180322 for 0000:00:0f.0 on minor O
ataz.00: ATAPI: UMuare Uirtual IDE CDROM Drive, 00000001, max UDMA/33
ataz.00: configured for UDMA/33

scsi 2:0:0:0: CD-ROM NECUMUar UMuare IDE CDR10 1.00 PQ: © ANSI: 5
cryptd: max_cpu_glen set to 1000

AUXZ version of gem_enc/dec engaged .

AES CTR mode byB optimization enabled

alg: No test for _gcm-aes-aesni (_driver-gcn-aes-aesni)

alg: No test for _generic-gcm-aes-aesni (_driver-generic-gcn-aes-aesni)
(PCI:66MHz:32-bit) 00:0c:29:89:66:35

. Intel(R) PRO/1000 Netuork Comnection

: [sdal 41943040 512-byte logical blocks: (21.4 6B/20.0 GiB)
Isdal Write Protect is off

Isdal Cache data unavailable

Isdal Assuning drive cache: urite through

sd 0:0:0:0: [sdal Attached SCSI disk

8021q: 802.10 ULAN Support ul.8

sr2 [sr0] scsid-nnc drive: 1x/1x uriter dud-ran cd/ru xasfornz cdda tray
cdron: Uniform CD-ROM driver Revision: 3.20
randon: fast init done

€1000: ens33 NIC Link is Up 1000 Mbps Full Duplex, Flow Control: None
IPu6: ADDRCONF(NETDEU_UP): ens33: link is not ready

adding ULAN 0 to HU filter on device ens33

IPu6: ADDRCONF (NETDEU_CHANGE) : ens33: link becomes ready

floppyd: no floppy controllers found
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localhost login:
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[root@localhost ~]# showmount -e 192.168.16.10
Export List for 192.168.10.10:

/nfs/share 192.168.10.0/24

[root@localhost ~1#

[root@localhost ~#

[root@localhost ~1# mkdir /mnt/nfs_client

[root@localhost ~I# mount -t nfs 132.168.10.10:/nfs/share /mnt/nfs_client
[root@localhost ~I# df -h | grep nfs

192.168.10.10:/nfs/share 176_6.56 11  38% /mnt/nfs_client
[root@localhost ~]# cat /mt/nfs_client/test. txt

hello NFS

[root@localhost ~1# vim /etc/fstab





