[image: image1.png]When not set, the global prefix (or @php_fpm prefix@) applies instead.
Note: This directive can also be relative to the global prefix.
Default Value: none

prefix = /path/to/pools/$pool

unix [E}/group of processes

; Note: The is mandatory. If the group is not set, the default
; will be used.
5 apache chosen to provide access to the same directories as httpd
nginx
; RPM: Keep a group allowed to write in log dir.
group = nginx
; The address on which to accept FastCGI requests.
; Valid syntaxes are:
; ‘'ip.add.re.ss:port’ - to listen on a TCP socket to a specific IPv4 address on
3 a specific port;
5 '[ip:6:addr:ess]:port’ - to listen on a TCP socket to a specific IPv6 address on
E a specific port;
5 port’ - to listen on a TCP socket to all addresses
E (IPv6 and IPva-mapped) on a specific port;
3 '/path/to/unix/socket’ - to listen on a unix socket.
; Note: This value is mandatory.

listen = 127.0.0.1:9000




[image: image2.png];| = 127.0.0.1:9000
= /var/opt/remi/php74/run/php-fpm/www. sock
; set (2) backlog.

Default Value: 511
backlog = 511

3 Set permissions for unix socket, if one is used. In Linux, read/write
permissions must be set in order to allow connections from a web server.
; Default Values: user and group are set as the running user

mode is set to @660
.owner = nginx
-group = nginx
-mode = 8660

When POSIX Access Control Lists are supported you can set them using
these options, value is a separated list of user/group names.
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